{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":13,"n_cols":5,"rows_kept":13,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[null,"Наименование Powerware","Расшифровка наименования.","ШхВхГ (мм)","(кг)"]
[]
["103004728-6591","Eaton PW9140 10KVA HARDWIRE 6U","ИБП Eaton Powerware 9140 10  кВА/8 кВт с внутренней батареей, вход/выход - клеммник,6U","430x263x760",115]
["103005093-6591","Eaton PW9140 7.5KVA HARDWIRE 6U","ИБП Eaton Powerware 9140 7.5 кВА/6 кВт с внутренней батареей, вход/выход - клеммник, 6U","430x263x760",115]
["103004729-6591","Eaton PW9140 3U EBM ","Внешняя доп батарея для ИБП Powerware 9140, 3U","430x131x660",80]
[]
[]
["116750221-001","X-slot: SNMP/Web","Web/SNMP адаптер "]
["116750224-001     ","Environmental Monitoring Probe (EMP)","Датчик температуры и влажности (для работы с Web/SNMP адаптером)"]
["103002510-5501   ","X-slot: Modus/Jbus","ModBus карта"]
[1018460,"X-slot: AS/400 relays","Карта \"сухих\" контактов AS/400"]
[1019017,"X-slot: Modem","Модемная карта"]
[103002143,"X-slot: RS232 port","Карта для соединения ИБП  через RS232 порт"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}